
/**************************************************************
 *
 * For this example, you need to install PubSubClient library:
 *   https://github.com/knolleary/pubsubclient
 *   or from http://librarymanager/all#PubSubClient
 *
 * TinyGSM Getting Started guide:
 *   https://tiny.cc/tinygsm-readme
 *
 * For more MQTT examples, see PubSubClient library
 *
 **************************************************************
 * This example connects to HiveMQ's showcase broker.
 *
 * You can quickly test sending and receiving messages from the HiveMQ webclient
 * available at http://www.hivemq.com/demos/websocket-client/.
 *
 * Subscribe to the topic GsmClientTest/ledStatus
 * Publish "toggle" to the topic GsmClientTest/led and the LED on your board
 * should toggle and you should see a new message published to
 * GsmClientTest/ledStatus with the newest LED status.
 *
 **************************************************************/

// Select your modem:
#define TINY_GSM_MODEM_SIM800
// #define TINY_GSM_MODEM_SIM808
// #define TINY_GSM_MODEM_SIM868
// #define TINY_GSM_MODEM_SIM900
// #define TINY_GSM_MODEM_SIM7000
// #define TINY_GSM_MODEM_SIM7000SSL
// #define TINY_GSM_MODEM_SIM7080
// #define TINY_GSM_MODEM_SIM5360
// #define TINY_GSM_MODEM_SIM7600
// #define TINY_GSM_MODEM_UBLOX
// #define TINY_GSM_MODEM_SARAR4
// #define TINY_GSM_MODEM_M95
// #define TINY_GSM_MODEM_BG96
// #define TINY_GSM_MODEM_A6
// #define TINY_GSM_MODEM_A7
// #define TINY_GSM_MODEM_M590
// #define TINY_GSM_MODEM_MC60
// #define TINY_GSM_MODEM_MC60E
// #define TINY_GSM_MODEM_ESP8266
// #define TINY_GSM_MODEM_XBEE
// #define TINY_GSM_MODEM_SEQUANS_MONARCH

// Set serial for debug console (to the Serial Monitor, default speed 115200)
#define SerialMon Serial

// Set serial for AT commands (to the module)
// Use Hardware Serial on Mega, Leonardo, Micro
#include <TinyGsmClient.h>
#include <PubSubClient.h>
#ifndef __AVR_ATmega328P__
HardwareSerial MySerial(1);
#define SerialAT MySerial

// or Software Serial on Uno, Nano
#else
#include <SoftwareSerial.h>
SoftwareSerial SerialAT(2, 3);  // RX, TX
#endif

// See all AT commands, if wanted
// #define DUMP_AT_COMMANDS

// Define the serial console for debug prints, if needed
#define TINY_GSM_DEBUG SerialMon

// Range to attempt to autobaud
// NOTE:  DO NOT AUTOBAUD in production code.  Once you've established
// communication, set a fixed baud rate using modem.setBaud(#).
#define GSM_AUTOBAUD_MIN 9600
#define GSM_AUTOBAUD_MAX 115200

// Add a reception delay, if needed.
// This may be needed for a fast processor at a slow baud rate.
// #define TINY_GSM_YIELD() { delay(2); }

// Define how you're planning to connect to the internet.
// This is only needed for this example, not in other code.
#define TINY_GSM_USE_GPRS true
#define TINY_GSM_USE_WIFI false

// set GSM PIN, if any
#define GSM_PIN ""

// Your GPRS credentials, if any
const char apn[]      = "CMNET";
const char gprsUser[] = "";
const char gprsPass[] = "";

// Your WiFi connection credentials, if applicable
const char wifiSSID[] = "YourSSID";
const char wifiPass[] = "YourWiFiPass";

// MQTT details
const char* broker = "broker.hivemq.com";

const char* topicLed       = "GsmClientTest/led";
const char* topicInit      = "GsmClientTest/init";
const char* topicLedStatus = "GsmClientTest/ledStatus";



// Just in case someone defined the wrong thing..
#if TINY_GSM_USE_GPRS && not defined TINY_GSM_MODEM_HAS_GPRS
#undef TINY_GSM_USE_GPRS
#undef TINY_GSM_USE_WIFI
#define TINY_GSM_USE_GPRS false
#define TINY_GSM_USE_WIFI true
#endif
#if TINY_GSM_USE_WIFI && not defined TINY_GSM_MODEM_HAS_WIFI
#undef TINY_GSM_USE_GPRS
#undef TINY_GSM_USE_WIFI
#define TINY_GSM_USE_GPRS true
#define TINY_GSM_USE_WIFI false
#endif

#ifdef DUMP_AT_COMMANDS
#include <StreamDebugger.h>
StreamDebugger debugger(SerialAT, SerialMon);
TinyGsm        modem(debugger);
#else
TinyGsm        modem(SerialAT);
#endif
TinyGsmClient client(modem);
PubSubClient  mqtt(client);

#define LED_PIN 13
int ledStatus = LOW;

uint32_t lastReconnectAttempt = 0;

void mqttCallback(char* topic, byte* payload, unsigned int len) {
  SerialMon.print("Message arrived [");
  SerialMon.print(topic);
  SerialMon.print("]: ");
  SerialMon.write(payload, len);
  SerialMon.println();

  // Only proceed if incoming message's topic matches
  if (String(topic) == topicLed) {
    ledStatus = !ledStatus;
    digitalWrite(LED_PIN, ledStatus);
    mqtt.publish(topicLedStatus, ledStatus ? "1" : "0");
  }
}

boolean mqttConnect() {
  SerialMon.print("Connecting to ");
  SerialMon.print(broker);

  // Connect to MQTT Broker
  boolean status = mqtt.connect("GsmClientTest");

  // Or, if you want to authenticate MQTT:
  // boolean status = mqtt.connect("GsmClientName", "mqtt_user", "mqtt_pass");

  if (status == false) {
    SerialMon.println(" fail");
    return false;
  }
  SerialMon.println(" success");
  mqtt.publish(topicInit, "GsmClientTest started");
  mqtt.subscribe(topicLed);
  return mqtt.connected();
}


void setup() {

  MySerial.begin(9600, SERIAL_8N1, 26, 14);
  // Set console baud rate
  SerialMon.begin(115200);
  delay(1010);

  pinMode(LED_PIN, OUTPUT);

  // !!!!!!!!!!!

  pinMode(32, OUTPUT);
  digitalWrite(32, HIGH);
  Serial.println("Wait...");    pinMode(25, OUTPUT);
  pinMode(33, OUTPUT);
  digitalWrite(33, LOW);
  delay(1800);
  Serial.println("Wait...1");

  digitalWrite(33, HIGH);
  // Set your reset, enable, power pins here
  // !!!!!!!!!!!
  Serial2.begin(9600);
  Serial.println("Wait...");
 // MySerial.begin(115200);
  delay(5000);
  MySerial.print("AT\r\n");
  MySerial.print("AT\r\n");
  MySerial.print("AT\r\n");
  MySerial.print("AT\r\n");
    String input = MySerial.readString();
  Serial.println(input);
    Serial.println("Wait..asdfasdf.");
  while (1)
  {
    input =MySerial.readString();
    Serial.println(input);
    MySerial.print("AT\r\n");
    delay(10);
  }
  
  
  delay(5000);
  

  //Serial2.begin(9600);
  //Serial2.print("AT\r\n");
  //delay(1000);
  
  //input = Serial2.readString();
  //Serial.println(input);

delay(16000);
  // Set GSM module baud rate
  TinyGsmAutoBaud(SerialAT, 9600, 460800);
  // SerialAT.begin(9600);
  delay(6000);

  // Restart takes quite some time
  // To skip it, call init() instead of restart()
  SerialMon.println("Initializing modem...");
 // modem.restart();
   modem.init();

  String modemInfo = modem.getModemInfo();
  SerialMon.print("Modem Info: ");
  SerialMon.println(modemInfo);

#if TINY_GSM_USE_GPRS
  // Unlock your SIM card with a PIN if needed
  if (GSM_PIN && modem.getSimStatus() != 3) { modem.simUnlock(GSM_PIN); }
#endif

#if TINY_GSM_USE_WIFI
  // Wifi connection parameters must be set before waiting for the network
  SerialMon.print(F("Setting SSID/password..."));
  if (!modem.networkConnect(wifiSSID, wifiPass)) {
    SerialMon.println(" fail");
    delay(10000);
    return;
  }
  SerialMon.println(" success");
#endif

#if TINY_GSM_USE_GPRS && defined TINY_GSM_MODEM_XBEE
  // The XBee must run the gprsConnect function BEFORE waiting for network!
  modem.gprsConnect(apn, gprsUser, gprsPass);
#endif

  SerialMon.print("Waiting for network...");
  if (!modem.waitForNetwork()) {
    SerialMon.println(" fail");
    delay(10000);
    return;
  }
  SerialMon.println(" success");

  if (modem.isNetworkConnected()) { SerialMon.println("Network connected"); }

#if TINY_GSM_USE_GPRS
  // GPRS connection parameters are usually set after network registration
  SerialMon.print(F("Connecting to "));
  SerialMon.print(apn);
  if (!modem.gprsConnect(apn, gprsUser, gprsPass)) {
    SerialMon.println(" fail");
    delay(10000);
    return;
  }
  SerialMon.println(" success");

  if (modem.isGprsConnected()) { SerialMon.println("GPRS connected"); }
#endif

  // MQTT Broker setup
  mqtt.setServer(broker, 1883);
  mqtt.setCallback(mqttCallback);
}

void loop() {
  // Make sure we're still registered on the network
  
}
